

Q)Configure DHCP within a LAN and outside LAN. ,.




Fig: Configuration within LAN





Ping Output:



4B)










Fig2: Configure DHCP outside LAN














Ping output:

