Q) Configure default route, static route to the Router.

Topology:







Fig: Default routing in router0











Commands:



Router0



Router1



Router2:



Ping output

